Simulated Radar Waveform and RF Dataset Generator for Incumbent Signals in the 3.5 GHz CBRS Band

“Software manual”

Communications Technology Laboratory

Wireless Networks Division

National Institute of Standards and Technology

Technical Contacts:

Dr. Raied Caromi, raied.caromi@nist.gov

Dr. Michael Souryal, souryal@nist.gov

This manual describes the usage of the waveform and RF dataset generator software tool and provides a glossary for all the parameters needed for the generation process.

***Software Disclaimer:***

NIST-developed software is provided by NIST as a public service. You may use, copy and distribute copies of the software in any medium, provided that you keep intact this entire notice. You may improve, modify and create derivative works of the software or any portion of the software, and you may copy and distribute such modifications or works. Modified works should carry a notice stating that you changed the software and should note the date and nature of any such change. Please explicitly acknowledge the National Institute of Standards and Technology as the source of the software.

NIST-developed software is expressly provided "AS IS." NIST MAKES NO WARRANTY OF ANY KIND, EXPRESS, IMPLIED, IN FACT OR ARISING BY OPERATION OF LAW, INCLUDING, WITHOUT LIMITATION, THE IMPLIED WARRANTY OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE, NON-INFRINGEMENT AND DATA ACCURACY. NIST NEITHER REPRESENTS NOR WARRANTS THAT THE OPERATION OF THE SOFTWARE WILL BE UNINTERRUPTED OR ERROR-FREE, OR THAT ANY DEFECTS WILL BE CORRECTED. NIST DOES NOT WARRANT OR MAKE ANY REPRESENTATIONS REGARDING THE USE OF THE SOFTWARE OR THE RESULTS THEREOF, INCLUDING BUT NOT LIMITED TO THE CORRECTNESS, ACCURACY, RELIABILITY, OR USEFULNESS OF THE SOFTWARE.

You are solely responsible for determining the appropriateness of using and distributing the software and you assume all risks associated with its use, including but not limited to the risks and costs of program errors, compliance with applicable laws, damage to or loss of data, programs or equipment, and the unavailability or interruption of operation. This software is not intended to be used in any situation where a failure could cause risk of injury or damage to property. The software developed by NIST employees is not subject to copyright protection within the United States.

See [NIST Software Disclaimer](https://www.nist.gov/disclaimer) for more details.

***Commercial Disclaimer:***

Certain commercial equipment, instruments, or materials are identified in this paper to foster understanding. Such identification does not imply recommendation or endorsement by the National Institute of Standards and Technology, nor does it imply that the materials or equipment identified are necessarily the best available for the purpose.

* **Waveform generation:**

The graphical user interface (GUI) consists of two tabs, Fig. 1 shows the waveform generation tab. The description of the parameters in this tab are summarized in Table 1.

A screenshot of a social media post

Description automatically generated

Fig. 1. Waveform generation example.

|  |  |  |
| --- | --- | --- |
| Parameter or function | Possible values | Description |
| Pulse Modulation | Pulse modulation type from Table 2. | Select pulse modulation type from drop down menu. |
| Sampling Frequency | A number > 2000 | The sampling frequency of the generated waveforms (Hz). |
| Number of Waveforms | Integer number | The number of the waveforms. |
| Use Parallel | N/A | Whether to use parallel processing in the generation process. |
| P0N#2 Phase Coding | Barker, Frank, P1, P2, P3, P4, Px, Zadoff-Chu | Select phase coding for pulse modulation type P0N#2. |
| Generate Waveforms | N/A | Generate a set of waveforms. For each pulse modulation, the other parameters (Pulse Width, Chirp Width, pulses per second, Pulses per Burst) are randomly selected with constraints from Table 1 for each bin. |
| Save waveforms | N/A | Save all generated waveforms in MATLAB cell format .mat file including generation parameters. |
| Show all parameters | N/A | Displays the generation parameters in a table. |

Table . Waveform generation glossary

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Pulse Modulation | Pulse Width (μs) | Chirp Width (MHz) | PRR (pulses per second) | Pulses per Burst (Min to Max) | Comments |
| P0N #1 | 0.5 to 2.5  Δ = 0.1 | N/A | 900-1100  Δ ≥ 10.0 | 15to 40  Min Δ = 5 | Similar to currently deployed Radar 1 |
| P0N #2 | 13-52  Δ = 13 | N/A | 300-3000  Δ ≥ 10.0 | 5 to 20  Δ ≥5 | Simulates possible phase-coded waveforms that could be used in future radar modulations |
| Q3N #1 | 3-5  Δ = 1.0 | 50-100  Δ = 10 | 300-3000  Δ ≥ 30 | 8 to 24  Δ ≥ 2 | Simulates possible future multi-function Q3N-type radar   * Short τ * Wide Bc |
| Q3N #2 | 10-30  Δ = 1.0 | 1-10  Δ = 1 | 300-3000  Δ ≥ 50 | 2 to 8  Δ ≥ 2 | Simulates possible future multi-function Q3N-type radar   * Intermediate τ * Intermediate Bc |
| Q3N #3 | 50-100  Δ = 5.0 | 50-100  Δ = 10 | 300-3000  Δ ≥ 100 | 8 to 24  Δ ≥ 2 | Simulates possible future multi-function Q3N-type radar   * Wide τ * Wide Bc |

Table . Proposed radar signal parameters for FCC 3.5 GHz ESC compliance testing*. NTIA Technical Memorandum 18-527 Available at* [*http://www.its.bldrdoc.gov/publications/3184.aspx*](http://www.its.bldrdoc.gov/publications/3184.aspx)*.*

* **Add Noise:**

The add noise tab in the GUI enables the addition of white Gaussian noise (WGN) and the generation of the dataset from the waveforms that were generated in the first tab. Fig. 1 and Fig. 2 show two examples of this process. The parameters in this tab are summarized in Table 3.

A screenshot of a cell phone

Description automatically generated

Fig. . Example of dataset generation with SNR range.

A screenshot of a cell phone

Description automatically generated

Fig. . Example of dataset generation with power level range.

|  |  |  |
| --- | --- | --- |
| Parameter or function | Possible values | Description |
| Load waveform Folder | N/A | Load waveforms from a folder. The folder may have more than one file. Usually many waveforms for each bin are saved in one file. The folder can have more than one file with same bin. |
| Noise power mode | Power Level Range, SNR Range | A method for how to set the power of the noise. After selecting one of these modes, the values in the next line changes according the mode. Power setting require measurement of radar peak power dBm per 1 MHz, and noise power dBm per 1 MHz. In all calculations, the reference load is assumed to be 1 ohm. |
| Power Level Range | Range of values (dBm/MHz) | The noise power is varied according to a range of values and each waveform noise level will be selected randomly from that range. On the other hand, the peak power of the radar is set at a fixed value dBm/MHz. |
| SNR Range | Range of values (dB) | The SNR is varied according to a range of values and each waveform SNR value will be selected randomly from that range. On the other hand, the noise power is set at a fixed value dBm/MHz. |
| Waveform duration | Keep, Fix to max, Fix to | Generally, the waveforms generated with this app has different durations due to the variations of the number of pulses per bursts and pulse repetitions between the bins. |
| Keep | N/A | keeps the duration of the original waveforms as is. |
| Fix to max | N/A | Fix the duration of the waveforms to the maximum duration of a waveform in the set. If a waveform has shorter duration, it is placed randomly at some time and the rest of samples are filled with noise. |
| Fix to | Number | Fix the waveform duration to a fixed value in (ms). If a waveform is longer, then it is trimmed from the end. On the other hand, if a waveform is shorter, it is placed randomly at some time from the beginning and the rest of the samples are filled with noise. |
| Include noise only set | N/A | Adds a subset of waveforms with noise only (no radar signal present) to the original waveform set. The number of noise only waveforms is equal to the number of the waveforms in the original set. The total number of waveforms is now double of the original set with half of them having no radar signal. |
| Signal center frequency | keep, set at, random | Select a method for the center frequency of the radar signal in the baseband. |
| keep | N/A | Do not change the center frequency (usually at zero Hz baseband). |
| Set at | Integer number | Set the center frequency at a specific value. |
| random | N/A | Set the center frequency at a random value. |
| Process Noise Addition | N/A | After setting all the parameters, click this button to add noise and create the dataset |
| Save method | One set, divide to subsets | How to save the waveforms in the dataset. |
| One set | N/A | Save all the waveforms in one dataset. |
| divide to subsets | N/A | Divide all the waveforms into multiple subsets according to subset size. |
| Subset size | Integer number | The size of the subset. |
| Convert subsets to arrays if possible | N/A | Convert the waveforms in the subset to one array instead of multiple MATLAB cell arrays. This is not possible if the waveforms have different durations. |
| Save dataset | N/A | Save the entire dataset to files. A popup dialog appears to set prefix names for the files and the variables of the dataset. |

Table . Add noise glossary

* **Requirements and limitations:**

The waveform generator requires enough free memory to process the generated set at once, or twice the size of the loaded waveform set when (include noise only set) check box is selected. The amount of the required memory dependents on the number of the waveforms, their sampling frequency, and the desired waveform duration. For parallel processing, the program requires multi cores. Parallel processing is only useful when generating very large datasets.

For example, a set of 5000 waveforms (1000 of each bin X 5 bins) sampled at 10 MHz and 80 ms long per waveform requires more than 60 GB of free memory for noise addition processing. If you don’t have enough the required resources, generate and process small sets of waveforms at each time.

* **Example of an RF dataset:**

A reference RF dataset was generated using this software. The RF dataset is published at <https://doi.org/10.18434/M32116>.

The dataset consists of four groups. The parameters for the groups are identical. The following table shows the parameters used for generating the reference dataset for one group.

|  |  |
| --- | --- |
| Parameter | Value |
| Pulse Modulation | P0N #1, P0N #2, Q3N #1, Q3N #2, Q3N #3 |
| Sampling Frequency (Hz) | 10000 |
| Number of Waveforms | 1000 for each pulse modulation type. |
| Generate Waveforms | Generate waveforms for each pulse modulation type separately. |
| Save waveforms | Save each pulse modulation type to the same folder after generation. |
| Load waveform Folder | Select the folder where the waveforms were saved ( 1000 for each pulse modulation type, 5000 total). |
| Noise power mode | SNR Range |
| SNR Range | 10 to 20, step 2. Scale noise power to -109 dBm/MHz. |
| Include noise only set | Check |
| Waveform duration | Fix to 80 ms |
| Save method | Divide to subsets |
| Subset size | 200 |
| Convert subsets to arrays if possible | Check |
| Signal center frequency | Random |
| Process Noise Addition | Click to process. |
| Save data Set | After finishing the process, click to save. |

Table . Dataset parameters for generating one group similar to the groups in the dataset “RF Dataset of Incumbent Radar Systems in the 3.5 GHz CBRS Band”